Chapter 1

Introduction

1.1 Introduction

1.2 Autonomous Vehicle

An independent car is too called a self-driving car or driverless car or automated car. Anything the title but the point of the innovation is the same. Down the memory line, independent vehicle innovation tests begun in 1920 as it were and controlled by radio technology. Later on, trails started in 1950. From the past few a long time, upgrading robotization innovation day by day and utilizing all perspectives of utilizing in regular human life. The display situation of human creatures is dependent to computerization and mechanical autonomy innovation utilizing like agriculture, medical, transportation, vehicle and fabricating businesses, IT division, etc. For the final ten a long time, the vehicle industry came forward to inquiring about independent vehicle innovation (Waymo Google, Uber, Tesla, Renault, Toyota, Audi, Volvo, Mercedes-Benz, General Engines, Nissan, Bosch, and Continental's independent vehicle, etc.). Level-3 Independent cars came out in 2020. Everyday autonomous vehicle innovation analysts are understanding challenges. In the future, without human offer assistance, robots will manufacture autonomous cars utilizing IoT innovation based on client prerequisites and Favor these vehicles are exceptionally secure and comfortable in transportation frameworks like human traveling or cargo. Independent vehicles require information and upgrading persistently, so in this case, IoT and Artificial insights offer assistance to share the data gadget to the gadget. This audit paper tended to what the innovations and strategies are utilized in independent vehicles by writing surveys and the hole between them.

Trajectory of a vehicle

The direction of a vehicle is a multifaceted concept including its spatial facilitates, speed, speeding up, and indeed twitch, all fastidiously depicted as capacities of time (Reference 1). It typifies the complicated exchange between the vehicle's development and the transient measurement, giving a comprehensive understanding of its way through space over a assigned period. In the setting of independent vehicles, direction arranging develops as a foremost endeavor, looking for to chart the most ideal course for the vehicle's route from its show area to a foreordained goal (Reference 2).

This arranging handle unfurls in the midst of a complex web of contemplations, where different variables such as deterrents, winning activity conditions, and the inborn flow of the vehicle come into play. By unpredictably analyzing these components, direction arranging calculations endeavor to strike a sensitive adjust between effectiveness, security, and consolation, guaranteeing a consistent and strong travel for the independent vehicle.

Moreover, the centrality of vehicle direction modeling expands past the domain of independent driving, serving as a foundational foundation for the improvement of urban brilliantly administrations (Reference 3). Through fastidious examination and modeling of vehicle directions, analysts and professionals pick up important bits of knowledge into optimizing transportation frameworks, improving security measures, and invigorating the in general effectiveness of urban landscapes.

By leveraging progressed computational methods and real-world information, direction modeling encourages the recreation and forecast of vehicle developments, empowering partners to expect and relieve potential challenges proactively. Moreover, this granular understanding of vehicle directions empowers the refinement of urban foundation and transportation approaches, cultivating economical and flexible urban situations competent of obliging the advancing needs of cutting edge society.

In substance, the direction of a vehicle rises above simple spatial development, epitomizing a wealthy embroidered artwork of worldly elements and vital decision-making. As independent vehicles proceed to multiply and reshape the texture of urban versatility, the craftsmanship and science of direction arranging and modeling will stay vital apparatuses in the journey for more secure, more astute, and more effective transportation frameworks.

ADAS

Progressed Driver-Assistance Frameworks are electronic frameworks that offer assistance the driver whereas driving the vehicle by giving exact perusing of the information collected from street environment utilizing different hardware to guarantee street security. When planned with a secure human-machine interface, they are aiming to increment driver security and generally street security. Most mishaps happen due to human mistake which can be effectively dodged by the utilize of fake insights along with electronic innovation. The ADAS are expecting to maintain a strategic distance from street mischances which ordinarily occur due to human blunder by utilizing electronic innovation. The utilize of this kind of framework in vehicles is awesome for applications like daze spot observing, lane-keep help and forward collision caution. The utilize of ADAS is a most to guarantee street security and appropriate activity management.[1]

Advanced driver-assistance frameworks (ADAS) are advances that help drivers with the secure operation of a vehicle. Through a human-machine interface, ADAS increment car and street security. ADAS utilize robotized innovation, such as sensors and cameras, to identify adjacent impediments or driver blunders, and react appropriately. ADAS can empower different levels of independent driving.[2]

Mixed Traffic Environments

Blended activity situations allude to roadways where different sorts of vehicles share the same space, counting conventional human-driven vehicles, bikes, cruisers, people on foot, and progressively, independent vehicles. These situations show interesting challenges and elements due to the contrasting speeds, sizes, behaviors, and vulnerabilities of the distinctive street. To securely and productively explore in complex urban activity, independent vehicles must make mindful forecasts in connection to encompassing traffic-agents (vehicles, bikes, people on foot, etc.). A challenging and basic assignment is to investigate the development designs of diverse traffic-agents and anticipate their future directions precisely to offer assistance the independent vehicle make sensible route decision.[1] Productive activity control can reduce activity clog, decrease fuel utilization, and move forward activity security. With the improvement of communication and robotization innovations, customary. vehicles (RVs), associated vehicles (CVs), and associated and mechanized vehicles (CAVs) will coexist on urban streets in the close future. [2] Heterogeneity is one of those characteristics which separate activity conditions of a creating nation from other created countries. The heterogeneity which speaks to the differing qualities among vehicle categories is suspected to have antagonistic impacts on path teach, blockage potential, and street users’ safety.[3]

Overview

Motivations

The motivations behind the study on trajectory prediction of vehicles in urban areas are multifaceted and address several critical aspects of autonomous vehicle technology and its integration into real-world settings.

Safety Enhancement: The primary motivation lies in improving the safety of autonomous vehicles operating in mixed traffic environments. By accurately predicting the trajectories of other road users, such as human-driven vehicles, cyclists, and pedestrians, autonomous vehicles can proactively anticipate and respond to potential collision scenarios.

Human-Autonomous Vehicle Interaction: In mixed traffic environments, human drivers often rely on implicit communication cues, such as eye contact and hand gestures, to negotiate interactions with other road users. Autonomous vehicles must be able to interpret and respond to these social cues effectively to navigate safely and smoothly. Therefore, the thesis aims to develop interactive trajectory prediction models that enable autonomous vehicles to anticipate and adapt to the behavior of human road users, fostering more natural and intuitive interactions on the road.

Traffic Flow Optimization: Effective trajectory prediction algorithms can contribute to optimizing traffic flow and reducing congestion in mixed traffic environments. By accurately forecasting the movements of different vehicles and anticipating potential bottlenecks or conflicts, autonomous vehicles can adjust their trajectories dynamically to minimize disruptions and maintain smooth traffic flow, thereby enhancing overall efficiency and mobility.

Real-World Deployment Challenges: Despite significant advancements in autonomous vehicle technology, deploying these vehicles in real-world environments poses numerous challenges, including unpredictable human behavior, complex traffic scenarios, and varying environmental conditions. By addressing the specific challenges of trajectory prediction in mixed traffic environments, the thesis aims to develop practical solutions that can facilitate the safe and efficient integration of autonomous vehicles into diverse urban and suburban settings.

Regulatory and Policy Implications: The successful deployment of autonomous vehicles hinges not only on technological advancements but also on regulatory frameworks and policy decisions that govern their operation. By providing insights into the capabilities and limitations of interactive trajectory prediction models, the thesis can inform policymakers and regulatory agencies in developing standards and guidelines for the safe and responsible deployment of autonomous vehicles in mixed traffic environments.

Overall, the thesis on interactive trajectory prediction of autonomous vehicles in mixed traffic environments is driven by the overarching goal of advancing the state-of-the-art in autonomous vehicle technology and accelerating the transition towards safer, more efficient, and more sustainable transportation systems. By addressing key challenges and opportunities in trajectory prediction, the research contributes to realizing the full potential of autonomous vehicles in reshaping the future of mobility.

Objectives

The objectives of the thesis on trajectory prediction of vehicles in urban areas are designed to address the complexities and challenges inherent in the integration of autonomous vehicles into real-world settings. These objectives encompass both technical advancements and practical applications, aimed at enhancing the safety, efficiency, and usability of autonomous vehicle technology in mixed traffic environments. The key objectives include:

Develop Accurate Trajectory Prediction Models: The primary objective is to develop advanced machine learning and predictive modeling techniques capable of accurately forecasting the trajectories of diverse road users, including human-driven vehicles, cyclists, and pedestrians. These models should incorporate factors such as historical data, environmental conditions, and social interactions to improve prediction accuracy and reliability.

Enhance Human-Autonomous Vehicle Interaction: Another objective is to enhance the interaction between autonomous vehicles and human road users by developing intuitive and socially-aware trajectory prediction algorithms. This involves analyzing and interpreting human behavior cues, such as gestures, eye contact, and body language, to anticipate and respond to the intentions of other road users effectively.

Improve Safety and Collision Avoidance: A key objective is to improve safety and collision avoidance capabilities of autonomous vehicles through proactive trajectory prediction and risk assessment. By accurately identifying potential collision scenarios and hazardous situations in advance, autonomous vehicles can take preemptive actions, such as adjusting speed or changing lanes, to mitigate risks and ensure safe navigation in mixed traffic environments.

Optimize Traffic Flow and Efficiency: The thesis aims to optimize traffic flow and reduce congestion in mixed traffic environments by developing trajectory prediction models that facilitate smoother interactions between autonomous vehicles and other road users. By dynamically adjusting trajectories based on real-time traffic conditions and congestion patterns, autonomous vehicles can contribute to improving overall traffic efficiency and mobility.

Validate and Evaluate Performance: An essential objective is to validate and evaluate the performance of the developed trajectory prediction models through extensive simulations and real-world testing scenarios. This involves assessing prediction accuracy, responsiveness, and reliability under diverse environmental conditions and traffic scenarios to ensure the robustness and effectiveness of the proposed approaches.

Overall, the objectives of the thesis are aligned with the overarching goal of advancing the state-of-the-art in autonomous vehicle technology and facilitating the seamless integration of autonomous vehicles into diverse urban and suburban landscapes. By addressing these objectives, the research contributes to realizing the potential benefits of autonomous vehicles in improving road safety, traffic efficiency, and mobility for society as a whole.

Challenges

The primary focus of this thesis revolves around the intricate task of trajectory prediction within a diverse and dynamic mixed traffic environment. This environment comprises various types of road agents, including but not limited to buses, trucks, motorcycles, pedestrians, and even animals. In addition to these diverse entities, the presence of traffic infrastructure elements such as traffic lights, traffic signs, and speed breakers further complicates the prediction task.

The challenges inherent in this scenario stem from the complex interactions and behaviors exhibited by the different road agents. Each type of agent possesses its own set of movement patterns, intentions, and responses to external stimuli. For instance, buses and trucks may have slower acceleration and deceleration rates compared to motorcycles, while pedestrians and animals exhibit unpredictable movements.

Furthermore, the dynamics of traffic signs and signals add another layer of complexity. Deciphering the intentions of road agents in response to these signals, such as stopping at a red light or yielding at a stop sign, requires a nuanced understanding of traffic rules and behavioral norms.

The ultimate goal of this thesis is to develop robust prediction models capable of accurately forecasting the trajectories of various road agents within this heterogeneous environment. These predictive capabilities are crucial for the successful implementation of autonomous driving systems and Advanced Driver Assistance Systems (ADAS). By effectively anticipating the movements of surrounding agents, autonomous vehicles can make informed decisions to ensure safe and efficient navigation through mixed traffic scenarios.

Thesis Organization

Conclusion

In this chapter, we've provided a comprehensive overview of the study to come, offering a preliminary look at the tasks that lie ahead. Through our discussion, we've highlighted the inspiration behind the research, articulated the objectives we seek to accomplish, and identified the challenges that will be further explored in subsequent chapters. By laying this groundwork, we've set the stage for a more in-depth examination of the motivations driving our inquiry, the specific goals we aim to achieve, and the obstacles we anticipate encountering. This introductory discussion serves as a foundation upon which we will build a deeper understanding of the complexities inherent in our research domain and the strategies required to address them effectively.

Chapter 2

Background Study

Introduction

**Deep** **Learning** **Model**

**LSTM**

Long short-term memory (LSTM) arrange is a repetitive neural organize (RNN), pointed at managing with the vanishing angle issue display in conventional RNNs. Its relative cold-heartedness to crevice length is its advantage over other RNNs, covered up Markov models and other grouping learning strategies. It points to give a short-term memory for RNN that can final thousands of timesteps, hence "long short-term memory".[1]

A common LSTM unit is composed of a cell, an input entryway, an yield gate[14] and a disregard gate.[15] The cell recollects values over self-assertive time interims and the three entryways control the stream of data into and out of the cell. Disregard doors choose what data to dispose of from a past state by relegating a past state, compared to a current input, a esteem between 0 and 1. A (adjusted) esteem of 1 implies to keep the data, and a esteem of 0 implies to dispose of it. Input doors choose which pieces of modern data to store in the current state, utilizing the same framework as disregard doors. Yield entryways control which pieces of data in the current state to yield by allotting a esteem from 0 to 1 to the data, considering the past and current states. Specifically yielding pertinent data from the current state permits the LSTM organize to keep up valuable, long-term conditions to make forecasts, both in current and future time-steps.

**CNN**

**GRU**

Conclusion

Chapter 3

Literature Review

Introduction

Within this literature review, an exploration unfolds surrounding the trajectory prediction of vehicles through the analysis of trajectories pertaining to diverse road agents, including buses, cars, and pedestrians. This examination traverses the landscape of machine learning and deep learning methodologies such as RNNs, CNNs, LSTMs, GANs, among others, employed for this purpose. Emphasizing the critical role of appropriate predictor variables, the review delves into discussions concerning potential advancements in predicting vehicle trajectories under varied conditions. Furthermore, it delves into the exploration of various optimization techniques, enriching the discourse surrounding this pivotal aspect of vehicular trajectory prediction.

Related Works

"TraPHic\_Trajectory\_Prediction.pdf" introduces a novel LSTM-CNN hybrid network for trajectory prediction in dense traffic scenarios. The paper addresses the limitations of existing models by incorporating factors such as velocity, turning radius, and local density to enhance prediction accuracy. By leveraging the strengths of both CNNs and LSTMs, the proposed model achieves a significant 30% improvement in accuracy on dense datasets, particularly showcasing its effectiveness on a new Asian urban dataset. Unlike traditional approaches, this model can handle heterogeneous road agents without explicit behavior assumptions, making it versatile for various traffic conditions.

The paper contributes to the field by bridging the gap in accurate trajectory forecasting, especially in dense traffic environments. While existing datasets like ApolloScape and NGSIM simulations offer diverse scenarios, this paper's approach provides a unique perspective on traffic prediction. By drawing inspiration from RNNs and LSTMs for sequence modeling, the model showcases the potential of combining different neural network architectures for more effective traffic prediction. However, the paper acknowledges limitations in the application of generative models like VAEs and GANs due to challenges in back-propagation during training. Despite this, the successful utilization of generative models for trajectory prediction in pedestrian crowds and sparse traffic scenarios demonstrates the paper's innovative contributions to the field.

----------------------------

The paper introduces TrafficPredict, a novel LSTM-based algorithm for predicting trajectories of heterogeneous traffic agents in urban environments. The main contribution lies in proposing a new approach to handle trajectory prediction scenarios where different types of traffic agents, such as vehicles, bicycles, and pedestrians, interact with each other. To model these interactions, the authors introduce a 4D graph structure that captures spatial and temporal relationships between agents, as well as similarities and differences between agent categories.

The proposed architecture consists of two main layers: an instance layer and a category layer. The instance layer aims to capture the movements and interactions of individual agents using LSTM networks and attention mechanisms. The category layer, on the other hand, learns the movement patterns and similarities of agents within the same category, providing guidance to refine the predictions for individual instances. By integrating information from both layers, the algorithm can leverage the collective knowledge of agent interactions and category-specific patterns.

To facilitate research in this area, the authors have collected and released a new large-scale trajectory dataset in urban traffic, featuring various traffic agents and interactions. Experimental results on this dataset demonstrate improved accuracy compared to previous state-of-the-art methods, with about 20% improvement in average displacement error and final displacement error.

Despite these contributions, the paper acknowledges some limitations. The accuracy of the proposed method may vary based on traffic conditions and the duration of observed past trajectories. Additionally, the method does not explicitly consider constraints such as lane directions, traffic signals, and traffic rules, which could potentially further improve prediction accuracy. The evaluation is also limited to a specific urban environment, and the performance may need to be validated in different traffic scenarios and environments. Furthermore, the paper does not provide a detailed comparison of computational efficiency and scalability with other methods, nor does it discuss the potential challenges in extending the method to handle a larger number of traffic agent categories or more complex interactions.

Overall, the paper presents a novel approach for trajectory prediction in heterogeneous traffic scenarios, contributing to modeling spatial and temporal relationships, learning category-specific patterns, and providing a new dataset for evaluation. However, there are opportunities for further improvements and validations in different traffic environments and conditions.

---------------------------------------

Recurrent Meta Neural network

The thesis paper titled "Interactive Trajectory Prediction for Autonomous Driving via Recurrent Meta Program Induction Network" by Chiyu Dong, Yilun Chen, and John M. Dolan presents a novel approach for predicting the trajectory of surrounding vehicles in autonomous driving scenarios. The authors highlight the importance of accurately predicting the future trajectories of neighboring vehicles for autonomous cars to interact and cooperate effectively in complex driving situations such as lane changes and merging.

The paper provides a comprehensive literature review of existing methods for interactive trajectory prediction and cooperative driving, categorizing them into rule-based, optimization-based, and probabilistic/learning approaches. The authors critique the limitations of these methods, such as the lack of consideration for interactions among vehicles, the need for manually designed probabilistic models and reward functions, and the inability to handle continuous action spaces or sequential information effectively.

The authors propose a Recurrent Meta Induction Network (RMIN) framework to address these shortcomings. The RMIN is based on the Conditional Neural Process (CNP), which uses a set of demonstration examples and an additional observation as inputs to predict the corresponding output. However, the original CNP does not consider the sequential information in the inputs due to permutation invariance requirements. The RMIN overcomes this limitation by replacing the original demonstration sub-net with a recurrent neural cell, allowing it to capture sequential information in the historical trajectories of surrounding vehicles.

The proposed method is evaluated on real trajectory data from the NGSIM dataset, specifically focusing on lane-change scenarios. The results demonstrate that the RMIN outperforms traditional kernel methods and the original CNP in terms of mean error in both longitudinal and lateral trajectory prediction. The authors attribute this improvement to the RMIN's ability to capture sequential information and the use of a fully connected network as the generator, which explicitly models the relationships among positions in the predicted trajectory.

Overall, the paper presents a novel and effective approach for interactive trajectory prediction in autonomous driving scenarios, addressing the limitations of existing methods and demonstrating its superiority through experimental results on real-world data.

------------------------

Driver Behavior Paper:

The paper starts with a comprehensive writing audit, covering considers on driving behaviors from the areas of social brain research and transportation inquire about. These thinks about have characterized drivers based on their levels of forcefulness and carefulness, regularly connecting these behaviors with components such as driver age, identity characteristics, and reactions to surveys. Be that as it may, the creators highlight the require for an approach that can recognize driver behaviors exclusively from sensor information, as would be required for independent driving systems.

The creators at that point examine earlier work related to direction highlights, independent car route, and adjustment to human driver behaviors. They distinguish restrictions in existing strategies, such as the failure to handle nonstop activity spaces, the require for physically outlined probabilistic models and remunerate capacities, and the need of thought for consecutive data in trajectories.

To address these confinements, the creators propose a novel set of direction highlights, counting a path taking after metric and a relative speed metric, that can be effortlessly extricated from vehicle directions. They conduct an expand web-based client ponder to build up a data-driven mapping between these highlights and six driver behaviors: forcefulness, carelessness, debilitating behavior, carefulness, cautiousness, and timidity.

Through figure investigation, the creators distinguish a inactive variable that summarizes these behaviors and can be utilized to degree the level of mindfulness required when driving close other vehicles. They join this mapping, called the Direction to Driver Behavior Mapping (TDBM), into an existing independent driving calculation, AutonoVi, to empower more secure real-time route by maintaining a strategic distance from possibly unsafe drivers.

The paper presents exploratory comes about illustrating the viability of the proposed approach in terms of made strides direction expectation exactness and more secure route choices compared to standard strategies.

---------------

Motion of road agent paper:

The paper presents a deep learning approach for predicting the future motion of vulnerable road users (VRUs) like pedestrians and bicyclists for autonomous driving applications. It builds upon recent work using rasterized images of the surrounding context as input to convolutional neural networks (CNNs) for motion prediction.

Traditional approaches for VRU motion prediction have relied on hand-crafted models like the social force model and Inverse Reinforcement Learning that attempt to encode interactions between actors and obstacles. However, the need to manually design features makes them difficult to scale to complex environments.

Many recent deep learning methods have applied recurrent models like LSTMs for motion prediction, incorporating factors like neighboring actor interactions through pooling or attention mechanisms. Some work has included static scene context by concatenating CNN features from scene images with actor states. However, most prior work does not fully leverage rich map data available in autonomous driving.

A key novelty of this paper is encoding high-definition map data like lane geometry, crosswalks, and traffic light states directly into the rasterized input images. The authors explore several variations of the rasterization pipeline and their impact, such as pixel resolution, rotating the frame to the actor's perspective, and different schemes for encoding map elements.

On the modeling side, the paper proposes a new efficient CNN architecture called FastMobileNet designed for fast inference speed on GPUs. It also introduces a spatial feature fusion technique to combine the rasterized context with other actor state features like velocity and acceleration.

Through extensive experiments, the authors demonstrate the benefits of their approach over baselines like unscented Kalman filters and Social-LSTM models, both in terms of prediction accuracy and inference speed. They also provide insights into which rasterization choices are most impactful for VRU prediction.

---------------------------

Map Driver Intention.pdf

The paper addresses the problem of estimating a driver's intended maneuver at road intersections for applications like advanced driver assistance systems and autonomous driving. It focuses on incorporating contextual information from digital maps and handling uncertain observations.

Previous work on maneuver intention estimation can be broadly categorized into discriminative and generative approaches. Discriminative methods like learning prototype trajectories from data are limited in generalizing to arbitrary intersections. Generative approaches explicitly model the process between intention and vehicle behavior, but often do not leverage map context.

Some works have used probabilistic representations like Bayesian filters, probabilistic finite state machines, and hierarchical hidden Markov models to model maneuver evolution. However, they either do not utilize map information or only consider topological characteristics like lane connectivity.

The European PReVENT-INTERSAFE project incorporated intersection topology but not geometry for probabilistic intention estimation. On the other hand, modeling approaches based on Gaussian processes have included geometric context like road borders, but assume accurate lane-level positioning which may not be realistic.

In contrast, the proposed approach uses a Bayesian network to probabilistically combine uncertain observations of the vehicle's behavior (position, orientation, turn signal) with both topological information like lane connectivity as well as geometric characteristics like lane shapes and paths extracted from a detailed digital map representation.

The key novelties are: 1) Jointly exploiting topological and geometric map context, and 2) Handling uncertainties in observations through virtual evidence in the Bayesian network instead of hard lane assignments. This allows reliable intention predictions even when the driver's behavior is inconsistent or ambiguous.

The method is evaluated on real traffic data, including scenarios with inconsistent driver behavior. A tailored evaluation procedure assesses if the system can reliably estimate maneuver intention when sufficient evidence is available while maintaining high uncertainty when observations are contradictory.

----------------

BAT

This thesis paper proposes a novel behavior-aware trajectory prediction model (BAT) for autonomous driving that incorporates insights from traffic psychology, human behavior, and decision-making. The authors highlight the critical need for accurate trajectory prediction of surrounding vehicles to enable fully autonomous driving.

The paper reviews prior work in trajectory prediction, categorizing approaches as physics-based, statistics-based, and deep learning-based. Physics-based methods use principles of physics and mechanics but often exhibit lower accuracy. Statistics-based approaches describe trajectories using predefined maneuver distributions and tend to perform better than physics-based ones. Deep learning methods like RNNs, CNNs, and Transformers have generally demonstrated superior performance, especially for long-term prediction.

The authors argue that mimicking human-like comprehension and response to surrounding traffic scenarios could be a breakthrough. They hypothesize that accounting for driver behaviors in the decision-making process of autonomous vehicles can enhance driving performance, motivating a deeper analysis of driver behavior for trajectory prediction.

The paper incorporates findings that drivers exhibit certain behavior patterns that are predictable, persistent, and consistent based on their driving styles. It also notes that humans tend to perceive their surroundings in relative terms like "slightly ahead and to the right" rather than absolute coordinates, suggesting polar coordinates may better represent human perception for trajectory prediction.

The proposed BAT model consists of behavior-aware, interaction-aware, priority-aware, and position-aware modules to capture driver behavior, vehicle interactions, relative importance of agents, and ego vehicle positioning respectively. A novel pooling mechanism using polar coordinates is introduced to align with human observation instincts.

The authors evaluate BAT across multiple real-world datasets (NGSIM, HighD, RounD, MoCAD) and show its superior performance over state-of-the-art baselines in terms of prediction accuracy and efficiency, even when trained on reduced data. Ablation studies confirm the importance of the key model components. Visualizations demonstrate BAT's ability to interpret driving behavior like humans for reliable trajectory predictions.

-------------------

Mixed Autonomy

The paper presents a novel trajectory prediction model called GaVa (Graph Attention for Vehicle Anticipation) for autonomous vehicles in mixed-autonomy traffic environments.

Traditional approaches to trajectory prediction have largely relied on computational methods like time-series analysis. In contrast, GaVa incorporates findings on how human drivers allocate visual attention based on factors like speed, proximity, and orientation. It introduces an "adaptive visual sector" mechanism that mimics how a driver's central field of view dynamically adjusts with speed.

The paper reviews prior work using deep learning for trajectory prediction, including Long Short-Term Memory (LSTM) networks, Convolutional Neural Networks (CNNs), and Graph Neural Networks (GNNs). Models combining CNNs and LSTMs or utilizing multi-head attention have shown promising results.

Research on visual behavior in driving is also covered, such as how a driver's visual field changes with speed, with slower speeds allowing a broader focus. Eye-tracking studies have confirmed drivers concentrate on the central region for vehicle control but shift attention for maneuvers like lane changes.

The proposed GaVa model contains several novel components inspired by this prior work: a Context-Aware Module for capturing temporal dependencies, an Interaction-Aware Module using CNNs and Graph Attention Networks to model spatial interactions between agents, a Vision-Aware Module incorporating an adaptive visual sector based on speed, and a Priority-Aware Module using a Transformer encoder-decoder for multi-trajectory prediction.

The authors evaluate GaVa on the NGSIM, HighD, and MoCAD datasets, outperforming state-of-the-art baselines by at least 15.2%, 19.4%, and 12.0% respectively across prediction horizons. Ablation studies validate the importance of components like the Interaction-Aware and Vision-Aware Modules.

**Conclusion:**

Previous literature reviews have predominantly concentrated on vehicle trajectory prediction, often employing a range of deep learning models and technologies for this purpose. Additionally, there exists literature exploring driver behavior and intentions while operating a vehicle, with a particular emphasis on the dynamics of different road agents. Nevertheless, much of the existing research tends to be narrowly focused on specific tasks within these domains. Recognizing this gap, I have formulated and executed my proposed methodology to offer a comprehensive approach to address these issues.

**Chapter 4**

**Proposed Methodology & Implementation**

**Introduction**


In the pursuit of accurately predicting the trajectories of road agents based on their temporal coordinates, the utilization of advanced deep learning techniques becomes imperative. Recurrent Neural Networks (RNNs) stand out as a formidable choice due to their innate ability to handle time series data efficiently. Specifically, the Gated Recurrent Unit (GRU), a variant of RNN, emerges as a pivotal component in our predictive framework.

Moreover, the incorporation of Convolutional Neural Networks (CNNs) enhances our predictive capabilities by extracting pertinent features from the dataset. This fusion of GRU and CNN architectures synergistically harnesses both temporal and spatial information, thereby enriching the predictive capacity of our model.

To further refine our predictive framework, we employ linear transformations for encoding and decoding, ensuring optimal information preservation throughout the prediction process. Additionally, meticulous preprocessing of the dataset is undertaken to organize homogeneous objects into structured numpy arrays. This preprocessing step not only enhances data organization but also lays a solid foundation for subsequent modeling endeavors.

Furthermore, the creation of trajectory and track arrays facilitates comprehensive data management and analysis, enabling seamless integration into our predictive pipeline. By adopting this meticulously crafted methodology, we aim to optimize model performance and elevate the accuracy and reliability of trajectory predictions.

**Methodology**

In the proposed methodology, we embrace a holistic approach to forecast the trajectories of diverse road agents. The journey commences with the collection of a meticulously curated dataset, followed by rigorous preprocessing procedures to refine and enhance its quality. Subsequently, we embark on the quest to identify salient features latent within the dataset, essential for informing our predictive model. To facilitate comprehensive analysis and experimentation, we partition the dataset into distinct subsets tailored for various objectives. Leveraging a custom deep learning model, meticulously tailored to the intricacies of the problem domain, we undertake the model training process. Once trained, the model undergoes rigorous testing, wherein its predictive capabilities are put to the ultimate trial. Through meticulous evaluation methodologies, we assess and quantify the performance of the model, shedding light on its efficacy and potential for real-world deployment.****

**Dataset** **Description**

Absolutely, here's a detailed description of the NGSIM dataset with its statistical size, source, attributes, and referencing:

**Source:**

* The NGSIM dataset originates from the Next Generation Simulation (NGSIM) program, a project by the U.S. Department of Transportation (DOT) [1].

**Data Collection:**

* The NGSIM program involved collecting real-world traffic data on four different highway locations in the United States [1]. These locations include:
  + US 101 (Los Angeles)
  + I-80 (Emeryville, California)
  + US 50 (Nevada)
  + I-66 (Virginia)

**Statistical Size:**

* The exact size of the NGSIM dataset varies depending on the specific data collection site and chosen data format. However, it generally contains data for thousands of vehicles over extended periods. Here's a reference for the size of a specific NGSIM dataset:
  + The I-80 dataset is reported to contain trajectory data for over 50,000 vehicles collected over a timeframe exceeding six weeks [2].

**Attributes:**

The NGSIM dataset includes various attributes for each vehicle, providing a comprehensive picture of the traffic scenario. Here are some key attributes:

* **Positional Data:**
  + X-coordinate (meters)
  + Y-coordinate (meters)
* **Motion Data:**
  + Speed (meters per second)
  + Acceleration (meters per second squared)
* **Vehicle Information:**
  + Lane identification
  + Vehicle type (e.g., car, truck)
* **Time Data:**
  + Timestamps for data collection

**Data Preprocessing**

Data preprocessing is a crucial step in preparing raw data for analysis, particularly in the context of machine learning applications. This process involves several key steps to enhance the quality and suitability of the data for specific analytical tasks. Let's break down the preprocessing steps described in your content:

Removing Null Values: The initial step involves identifying and removing null or missing values from the NGSIM dataset. Null values can introduce inconsistencies and inaccuracies in the data, potentially affecting the performance of machine learning models.

Filtering Objects by Type: The data is further preprocessed by filtering out specific classes of objects based on their type attribute. This typically involves segregating objects into categories such as vehicles, bikes/motorcycles, and humans. Separate arrays are then created to store trajectories for each class, enabling focused analysis on particular types of road agents.

Storage of Preprocessed Data: The preprocessed trajectory data is stored in NumPy binary files, providing an efficient and structured format for subsequent analysis. These files encapsulate the cleaned and transformed data, ensuring its integrity and accessibility for machine learning tasks.

Creation of Track Arrays: Additionally, numpy arrays are generated to create tracks for specific types of road agents. This involves aggregating the positions of a particular object in each frame of the dataset, enabling the reconstruction of its trajectory over time. These track arrays provide valuable context for understanding the movement patterns and behaviors of different road agents.

Calculation of Distance and Vehicle Attributes: Various metrics, such as distance from the ego vehicle to other vehicles, length, speed, and acceleration of vehicles, are calculated as part of the preprocessing pipeline. These metrics offer insights into the spatial relationships and dynamics of vehicles within the environment, enriching the dataset with additional features for machine learning analysis.

Data Saving: Finally, the preprocessed data, including trajectory arrays, track arrays, and calculated vehicle attributes, is saved to files for future reference and analysis. This ensures the preservation of the processed data in a structured and accessible format, ready for utilization in machine learning models and experiments.

By following these preprocessing steps, the raw NGSIM dataset is transformed into a cleaned, organized, and enriched dataset, primed for effective analysis using machine learning techniques.

**Feature Extraction**

The technique used to extract features in this code snippet is primarily based on calculating the distances and positions of surrounding obstacles relative to the main object (e.g., vehicle) in each trajectory. Here's a general overview of the feature extraction process:

Identifying Surrounding Objects: For each frame of the trajectory, the code identifies nearby objects or obstacles within the environment. These could include other vehicles, pedestrians, or any other relevant entities.

Calculating Relative Positions: Once the surrounding objects are identified, the code computes the relative positions of these objects with respect to the main object (e.g., the vehicle of interest). This typically involves calculating the differences in x and y coordinates between the main object and each surrounding object.

Calculating Distances: After determining the relative positions, the code computes the distances between the main object and each surrounding object. This is often done using formulas such as Euclidean distance or squared distance.

Organizing Features: The extracted features, such as distances and positions, are then organized into different categories based on their spatial relationships (e.g., left-top, center-bottom) with respect to the main object.

Feature Representation: Finally, the extracted features are represented in a structured format, typically as arrays or matrices, and stored for further analysis or processing.

While the code snippet does not explicitly provide the exact formulas or techniques used for feature extraction, it likely involves basic geometric calculations to determine distances and positions between objects in the environment. These calculations enable the characterization of the spatial relationships between the main object and surrounding obstacles, which is crucial for tasks such as object detection, tracking, and motion prediction in dynamic environments.

**Training Set and Testing Set**

In this scenario, the goal is to effectively manage trajectory data by partitioning it into distinct subsets for training, validation, and testing purposes. The process begins by aggregating trajectory data from multiple files, ensuring a comprehensive dataset for analysis. To maintain data integrity, trajectories are segregated based on unique vehicle identifiers, ensuring that each subset retains the complete trajectory history of individual vehicles.

Following this, a train-test split is performed to allocate data for training and testing the machine learning models. Here, 80% of the data is assigned to the training set, while the remaining 20% is reserved for testing. However, to further enhance model performance and prevent overfitting, the training set undergoes additional partitioning. Approximately 12.5% of the training data is set aside as a validation set, serving as an independent dataset to fine-tune model parameters and evaluate its performance during training.

To facilitate efficient data management and analysis, trajectory and track data structures are constructed for each subset. These structures enable the organization and storage of trajectory information, ensuring easy access and manipulation during model development and evaluation. Finally, the partitioned data is saved in both text and NumPy binary formats, providing flexibility and compatibility for subsequent machine learning tasks.

Overall, this meticulous partitioning process ensures that trajectory data is appropriately utilized for training, validation, and testing machine learning models, ultimately enhancing their accuracy and reliability in real-world applications.

**Model Architecture**

**A diagram of a process

Description automatically generated**

Certainly! Here's a description of the purpose of each layer in the provided neural network architecture:

1. Input Embedding: The purpose of these layers is to transform the input features into a lower-dimensional space, which helps in capturing essential information and reducing the complexity of the model.

2. Encoder: This layer encodes the temporal sequence of input features, capturing the dependencies and patterns over time in the trajectory data.

3. Vehicle Dynamics Embedding: This layer extracts a representation of vehicle dynamics from the encoded features, providing insights into the dynamic behavior of the agents.

4. Batch Normalization: Batch normalization layers normalize the activations of the previous layer, making training more stable and accelerating convergence by reducing internal covariate shift.

5. Optional Behavioral Modification: If enabled, this layer adjusts the weights of the encoder GRU’s hidden vectors based on additional information, potentially enhancing the model’s performance in capturing specific behaviors.

6. Convolutional Social Pooling and Embedding: These layers capture social interactions among agents in the scene by applying convolutional operations followed by max-pooling. They help the model understand the spatial relationships and interactions among different agents.


7. Decoder: This layer decodes the encoded features and predicts future trajectories based on the learned representations. It generates sequential outputs while considering contextual information from the encoder and social embeddings.

8. Output Layers: These layers produce the final predictions of the model. They generate outputs such as position coordinates and maneuver classes, enabling the model to forecast the future trajectories of road agents.

9. Dropout: Dropout regularization is applied to prevent overfitting by randomly dropping a fraction of the neurons during training, promoting the generalization of the model.

10. Activation Functions: These functions introduce non-linearity into the model and transform the outputs into suitable formats, such as probabilities for categorical predictions or positive values for continuous predictions.

**Hybrid Model**

In this section, we introduce our innovative network architecture designed for trajectory prediction within dense and heterogeneous traffic environments. In the context of heterogeneous traffic, the objective is to forecast trajectories, representing temporal sequences of spatial coordinates for a given road agent. Predicting temporal sequences demands models capable of capturing temporal dependencies within data, such as Gated Recurrent Units (GRUs). However, traditional GRUs operate independently for each road agent, failing to learn dependencies or relationships among heterogeneous agents. To address this limitation, we integrate Convolutional Neural Networks (CNNs) to identify interactions among different road agents. By combining CNNs with GRUs, our architecture learns locally significant relationships, both spatially and temporally, among heterogeneous road agents. The architecture comprises three map:

1. Horizon Map: Processes embeddings of agents within the "horizon" or semi-elliptical region ahead of the target agent. These embeddings traverse Fully Connected (FC) layers and GRUs to construct a "horizon map".

2. Neighbor Map: Handles embeddings of agents neighboring the target agent. Similar to the horizon layer, these embeddings pass through FC layers and GRUs to form a "neighbor map".

3. Ego Agent: Focuses on the embedding of the target agent itself, processing it through FC and GRU layers.

This integrated approach enables our model to effectively capture intricate interactions and dependencies among heterogeneous road agents, thereby enhancing trajectory prediction accuracy in complex traffic scenarios.

**Conclusion**

This chapter comprehensively addresses the foundational components pivotal to our proposed deep learning methodology, emphasizing dataset characteristics, data pre-processing techniques, feature extraction methodologies, and the creation of training and testing sets. Furthermore, it delves into detailed insights regarding the architecture of the hybrid model, shedding light on the composition and functionality of individual layers. By elucidating these essential elements, this chapter provides a comprehensive understanding of the methodological framework underpinning our approach. Through meticulous dataset description, rigorous pre-processing protocols, and sophisticated feature extraction strategies, we ensure the robustness and efficacy of our model. Additionally, the delineation of training and testing set creation methodologies underscores the meticulousness applied in model evaluation. Moreover, the exposition of model layer information offers valuable insights into the inner workings and structural intricacies of our hybrid architecture. Overall, this chapter serves as a conclusive synthesis of the methodological framework, laying the groundwork for subsequent experimental investigations and analytical assessments.